Link Budget

LED Power – 12.4 uW

Power after Fibre – 4.5 uW

Power Loss in dB - -4.4 dB

Power Required for detection – 1 uW

Power overhead – 6.5 dB, 3.5 uW